;;	EditText.dat
;;
;; 2005/8/19

[SELECT_PARTS_DIALOG]
COUNT=1
TEXT1=Select your replaced or removed part(s), and detemine with OK button so that all of required adjustments will automatically be decided, and guide you in correct order.

[STATUS_MONITOR]
BitmapFile1=prnidle.bmp
BitmapFile2=prnerror.bmp

[INDIVIDUAL_LIST]
COUNT=1
TEXT1=Select an adjustment item from the below window. Then, double-click your target adjustment item to execute it.

[EEPROM_COPY]
COUNT=4
TEXT1=This function copies EEPROM data from current main board to new main board.
TEXT2=1) Click [Backup] button to backup EEPROM data from current main board.
TEXT3=2) Turn off the printer and replace current main board with new one.
TEXT4=3) Trun on the printer again and click [Restore] button.

[EEPROM_INITIALIZE]
COUNT=5
TEXT1=NOTE : Please don't execute this function when backing up the EEPROM data
TEXT2=       with EEPROM Data Copy function.
TEXT3=
TEXT4=1) Input the Product Serial No. and click [Initial setting] button to write initial setting value to EEPROM.
TEXT5=2) Click the [Check] button to read out current setting values.

[HEAD_ID_INPUT]
BitmapFile1=headid.bmp
COUNT=7
TEXT1=[How to input Head ID]
TEXT2=1) Input Head ID on edit box.
TEXT3=2) Click [Input] button to register Head ID into EEPROM.
TEXT4=     If error message is displayed, please input Head ID again.
TEXT5=
TEXT6=[How to check current Head ID]
TEXT7=1) Click [Check] button to check current Head ID.

[TOF_ADJUSTMENT]
COUNT=5
TEXT1=1) Set A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Measure the distance between the edge of paper and printed line.
TEXT4=4) Select the proper adjustment value from the measurement result.
TEXT5=5) Click [Input] button to register the selected value into EEPROM.

[TOF_ADJUSTMENT]
COUNT=9
TEXT1=1) Set A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Measure the distance between the edge of paper and printed line.
TEXT4=4) Select the proper adjustment value from the measurement result.
TEXT5=5) Click [Input] button to record the selected value into EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=T.B.D
TEXT9=Refer to service manual

[HEAD_ANGULAR]
COUNT=9
TEXT1=1) Set A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern. 
TEXT3=3) Select the best pattern from each check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.
TEXT6=     In case that there is no best pattern, you have to input the maximun or 
TEXT7=     mininum parameter in the check pattern once. Due to this, the check pattern
TEXT8=     with offset value is printed in the center position of next check pattern print.
TEXT9=     Please repeat this adjustment until you can select the best pattern.

[MANUAL_BID]
COUNT=9
TEXT1=1) Set A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern of selected dot size.
TEXT3=3) Select the best pattern from each check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.
TEXT6=     In case that there is no best pattern, you have to input the maximun or 
TEXT7=     mininum parameter in the check pattern once. Due to this, the check pattern
TEXT8=     with offset value is printed in the center position of next check pattern print.
TEXT9=     Please repeat this adjustment until you can select the best pattern.

[PF_BAND_ADJUSTMENT]
COUNT=5
TEXT1=1) Set A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the best pattern from the check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.

[CLEANING]
COUNT=4
TEXT1=1) Click [Print] button to print nozzle check pattern print.
TEXT2=2) If dot missing appers, click [Cleaning] button to perform the cleaning.
TEXT3=3) Click [Print] button to print nozzle check pattern print again.
TEXT4=4) If dot mssing is not recovered, repeat from step 2) to step 3) 

[INK_CHARGE]
COUNT=5
TEXT1=1) Click [Ink Charge] button to perform ink charge.
TEXT2=2) Click [Print] button to print nozzle check pattern print.
TEXT3=3) If dot missing appers, click [Cleaning] button to perform the cleaning.
TEXT4=4) Click [Print] button to print nozzle check pattern print again.
TEXT5=5) If dot mssing is not recovered, repeat from step 3) to step 4) 

[INK_PAD_COUNTER]
COUNT=6
TEXT1=NOTE : You have to replace waste ink pad with new one once you initialize
TEXT2=             the protection counter.
TEXT3=
TEXT4=1) Click [Check] button to check current protection counter.
TEXT5=2) Replace waste ink pad with new one.
TEXT6=3) Click [Initialization] to reset current protection counter.

[SHIPPING_SETTING]
COUNT=5
TEXT1=This function will have a cleaning process performed automatically when the printer is turned on.
TEXT2=1) Please implement this function in case of nozzle expulsion troubles caused by the transport. When clicking the "Write" button, the shipping settings are entered in the machine.
TEXT3=2) The shipping settings will be registered when the printer is turned off and applied directly the next time it is turned on.
TEXT4=Attention:
TEXT5=The function resets the shipping settings if the printer is turned on. In this situation, it is necessary to implement the shipping settings once again before turning off the power.

[CHECK_PATTERN_PRINT]
COUNT=1
TEXT1=1) Click [Print] button to print selected pattern.

[EEPROM_READOUT]
COUNT=1
TEXT1=1) Click [Dump] button to read out and save all of EEPROM data.

[OPERATION_INFO]
COUNT=1
TEXT1=1) Click the [Check] button to read out the printer information.

[INK_DISCHARGE]
COUNT=4
TEXT1=1) Use the Jig.
TEXT2=2) Use the shipping liquid (CR02)
TEXT3=3) Click the [Perform] button to start the discharge.
TEXT4=4) Please discharge the shipping liquid outside of the printer when you execute this function.Otherwise ink may possible leak from the waste ink pad at user side.

[PAPER_FEED_TEST]
COUNT=1
TEXT1=1) Set the number of sheets. And click [Perform] buttont.
